# Supported Intel® PRO/1000 Server Adapters and Connections

This driver and software are designed to operate with the following Intel® PRO/1000 Server Adapters:

Product Name | Distinguishing Features | Board ID #† | Controller
--- | --- | --- | ---
Intel® PRO/1000 PT Server Adapter | PCI-E, Copper RJ45 connectors, supports 10/100/1000 | D15983-xxx | 82572EI
Intel® PRO/1000 PF Server Adapter | Fiber LC connectors, SX optics, 850nm, multimode | D16148-xxx | 82572EI
Intel® PRO/1000 PT Network Connection | Copper RJ45 connectors, supports 10/100/1000 | n/a | 82572EI
Intel® PRO/1000 PF Network Connection | Fiber LC connectors, SX optics, 850nm, multimode | n/a | 82572EI
Intel® PRO/1000 PB Server Connection | Copper RJ45 connectors, supports 10/100/1000 | n/a | 82572EI
Intel® PRO/1000 PF Dual Port Server Adapter | PCI Express, Fiber LC connectors, SX optics, 850nm, multimode | C60719-xxx | 82571EB
Intel® PRO/1000 PT Dual Port Server Adapter | PCI Express, Copper RJ45 connectors, supports 10/100/1000 | C49041-xxx | 82571EB
Intel® PRO/1000 PT Dual Port Network Connection | Copper RJ45 connectors, supports 10/100/1000 | n/a | 82571EB
Intel® PRO/1000 PF Dual Port Server Connection | Fiber LC connectors, SX optics, 850nm, multimode | n/a | 82571EB
Intel® PRO/1000 GT Dual Port Server Adapter | Copper RJ45 connectors, supports 10/100/1000 | C82381-xxx | 82545GM
Intel® PRO/1000 P Dual Port Server Adapter | PCI-Express, Copper RJ45 connectors, supports 10/100/1000 | C87216-xxx | 82546GB
Intel® PRO/1000 MT Quad Port Server Adapter | Copper RJ45 connectors, supports 10/100/1000 | C32199-xxx | 82546EB
Intel® PRO/1000 MT Dual Port Server Adapter | Copper RJ45 connectors, supports 10/100/1000 | A92111-xxx C29887-xxx C41421-xxx | 82545EB 82545GB
Intel® PRO/1000 MT Server Adapter | Copper RJ45 connector, supports 10/100/1000 | A92165-xxx C31527-xxx C36840-xxx | 82545EM 82545GM
Intel® PRO/1000 MF Dual Port Server Adapter | Fiber LC connectors, SX optics, 850nm, multimode | A91620-xxx C30848-xxx C41300-xxx | 82546EB 82545GB
Intel® PRO/1000 MF Server (LX) Adapter | Fiber LC connector, LX optics, 1310nm, long-haul single-mode | A91624-xxx C33916-xxx C37793-xxx | 82545EM 82545GM
Intel® PRO/1000 MF Server Adapter | Fiber LC connector, SX optics, 850nm, multimode. | A91622-xxx C33915-xxx C36851-xxx | 82545EM 82545GM
Intel® PRO/1000 XT Server Adapter | Copper connector, supports 10/100/1000 | A51580-xxx | 82544EI
Intel® PRO/1000 XF Server Adapter | Fiber SC connector, SX optics, 850nm, multimode | A50484-xxx | 82544EI
Intel® PRO/1000 T Server Adapter | Copper RJ45 connector, supports 10/100/1000 | A19845-xxx A33948-xxx | 82543GC
Intel® PRO/1000 F Server Adapter | Fiber SC connector, SX optics, 850nm, multimode | 738640-xxx A38888-xxx | 82543GC
Intel® PRO/1000 CT Network Connection | Copper RJ45 connector, supports 10/100/1000 | n/a | 82547GI
Intel® PRO/1000 MB Dual Port Server Connection | Copper RJ45 connectors, supports 10/100/1000 | n/a | 82546GB
Intel® PRO/1000 MB Dual Port Network Connection | Copper RJ45 connectors, supports 10/100/1000 | n/a | 82546GB
Intel® PRO/1000 MB Server Connection | Fiber connection, 850nm, multimode | n/a | 82545GM
Intel® PRO/1000 MT Server Connection | Copper connection, supports 10/100/1000 | n/a | 82545GM
Intel® PRO/1000 MT Network Connection | Copper connection, supports 10/100/1000 | n/a | 82545EM
Intel® PRO/1000 MF Dual Port Network Connection | Fiber SC connector, SX optics, 850nm, multimode | n/a | 82546EB

†Board ID # = A 6-digit code with a 3-digit extension; printed on barcode sticker on the front of the card.

See the Adapter & Driver ID Guide: http://support.intel.com/support/network

A "Network Connection" is a networking feature built into the motherboard. Thus, no board IDs. LED placement is at the discretion of the motherboard manufacturer.

### Compatibility Notes

Intel's first generation PRO/1000 Gigabit Server Adapter has the following limitations:

- Virtual LANs on this adapter are supported only in Microsoft* Windows* 2000, Windows XP, and Windows Server* 2003.

- Jumbo Frames on this adapter are not supported under Linux.

- This adapter operates correctly in 32- and 64-bit slots. However, when inserted in a 64-bit PCI slot, it will incorrectly indicate that it is in a 32-bit slot.

- This adapter does not support packet tagging for Quality of Service or Virtual LANs.

`Last modified on 9/19/05 2:52p Revision 14`