# Jumbo Frames

Jumbo frames are Ethernet frames that are larger than 1518 bytes. You can use Jumbo Frames to reduce server CPU utilization and increase throughput. However, additional latency may be introduced.

| NOTES: Jumbo Frames are supported at 1000 Mbps and 10Gbps. Using Jumbo Frames at 10 or 100 Mbps may result in poor performance or loss of link. End-to-end network hardware must support this capability; otherwise, packets will be dropped.

Jumbo Frames can be implemented simultaneously with VLANs and teaming.

To configure Jumbo Frames at the switch, consult your network administrator or switch user's guide.

Restrictions:

- Jumbo frames are not supported in multi-vendor team configurations.

- Supported protocols are limited to IP (TCP, UDP).

- Jumbo frames require compatible switch connections that forward Jumbo Frames. Contact your switch vendor for more information.

- When standard sized Ethernet frames (64 to 1518 bytes) are used, there is no benefit to configuring Jumbo Frames.

- The Jumbo Frames setting on the switch must be set to at least 8 bytes larger than the adapter setting for Microsoft* Windows* operating systems, and at least 22 bytes larger for all other operating systems.

- The Intel® PRO/1000 PM Network Connection does not support jumbo frames.

- The Intel® PRO/1000 PT Server Adapter, Intel® PRO/1000 PF Server Adapter, Intel® PRO/1000 PT Network Connection, Intel® PRO/1000 PF Network Connection, Intel® PRO/1000 PB Server Connection, Intel® PRO/1000 PF Dual Port Server Adapter, Intel® PRO/1000 PT Dual Port Server Adapter, Intel® PRO/1000 PF Dual Port Server Connection, and Intel® PRO/1000 PT Dual Port Network Connection do not support jumbo frames larger than 10500 bytes.

`Last modified on 8/31/05 4:17p Revision 4`