# Example NetWare* Configuration Files for ANS.

Here is a series of examples for common configurations of Intel's intermediate driver software, iANS.LAN. These examples use a combination of Intel PRO/1000 and PRO/100 adapters. The intermediate driver uses the same syntax with all Intel server adapters regardless of speed. Therefore you may substitute CE100B for E1000/E1000E and vice versa in any of these examples. The only exception to this is that EtherChannel keywords are dependent on the connection speed. Use "mode=fec" for 10 or 100 Mbps and "mode=gec" for gigabit connections.

1. Example 1: Two-Adapter AFT Team
   1 PRO/1000 server and 1 PRO/100 server adapter - Ethernet_802.2 frame type, IPX protocol.

2. Example 2: Two- Adapter ALB Team
   2 PRO/1000 server adapters - Ethernet_II frame type, IP and IPX protocols.

3. Example 3: Teaming
   2 PRO/1000 server adapter Static Link Aggregation team - 2 frame types, IP and IPX protocols.
   4 PRO/100 server adapters in a IEEE 802.3ad team.

4. Example 4: One Adapter, 2 VLANs
   1 PRO/1000 server adapter - Ethernet_II frame type, IP protocol.

5. Example 5: One Adapter, 3 VLANs
   1 PRO/100 server adapters - All 4 frame types, IPX protocol.

6. Example 6: Two- Adapter ALB Team, 5 VLANs
   2 PRO/1000 server adapters - Ethernet_II, IP and IPX protocols.

7. Example 7: Two Teams
   1 PRO/1000 server and 1 PRO/100 server adapter Static Link Aggregation team - 2 frame types, IP and IPX protocols.
   1 PRO/100 server adapter, 2 VLANs - 2 frame types, IP and IPX protocols.

Return to NetWare teaming instructions

`Last modified on 9/08/05 7:12a Revision 5`