# Configuring VLANs in Microsoft* Windows*

In Microsoft* Windows*, you must use Intel® PROSet to set up and configure VLANs. For more information, select Intel PROSet in the Table of Contents (left pane) of this window.

The following versions of Microsoft Windows support Intel PRO adapters when configured for VLANs:

- Windows 2000 (with Service Pack 4 or later)

- Windows XP

- Windows Server* 2003

In most environments, a maximum of 64 VLANs per server are supported by Intel PROSet.

Intel PRO Adapters do not support VLANs on Microsoft Windows 98.

`Last modified on 8/31/05 4:09p Revision 6`