# Novell NetWare* DOS ODI Client Driver Installation

Tips

Sample Files

Command Line Parameters

## VLM Installation

This version of E100BODI.COM requires latest version of the VLM client (version 1.21 or greater).

Refer to the Novell NetWare documentation for complete installation instructions.

## Tips (DOS ODI)

- In CONFIG.SYS, add the line LASTDRIVE=Z. In NET.CFG, under the NetWare DOS REQUESTER section (indented), add the line FIRST NETWORK DRIVE=<the first unused drive letter>.

- Support for promiscuous mode is not available as ASM does not include a receive monitor stack. If needed, load RXMONSTK.COM from the VLM client kit. RXMONSTK.COM should be loaded before E100BODI.COM and after LSL.COM in autoexec.bat.

- If running EMM386, make sure you are using v4.49 or later (ships with DOS 6.22).

## Sample Files

AUTOEXEC.BAT:

CD\NWCLIENT
LSL
E100BODI
IPXODI
NETX (or VLM optional)

CONFIG.SYS:

DEVICE=C:\WINDOWS|HIMEM.SYS
BUFFERS=30,0
FILES=60 (This can be set to more than 60 to improve performance.)
LASTDRIVE=Z (for NETX LASTDRIVE=F or first available drive letter)

NET.CFG:

LINK DRIVER E100BODI
FRAME ETHERNET_802.2
PROTOCOL IPX EO Ethernet_802.2
NETWARE DOS REQUESTER
FIRST NETWORK DRIVE = F

`Last modified on 9/08/05 7:12a Revision 3`