# Express Teaming

Express Teaming is a quick way to team together all of the ports of a multi-port Adapter on Microsoft* Windows* 2000, Windows XP, and Windows Server* 2003. Express Teaming is built into the base driver and does not require any other software.

## Setting Up Express Teaming

Install the driver (Intel® PROSet is optional, support for Express Teaming is built into the base driver). You can set up an Express Team the Advanced tab of the adapter's Properties (if you have Intel® PROSet for Windows* Device Manager installed, Express Teaming is on the Teaming tab). For information about installing drivers and Intel PROSet, select the appropriate topic in the Table of Contents (left pane of this window).

| NOTE: Do not uninstall an Express Team by right-clicking on it in device manager. Uninstall Express Teams only through adapter properties.

#### Waking Up a System

An Express Team can wake up the system it is in if it has "Allow this device to bring the computer out of standby" enabled in the Power Management Property Page. In order for this functionality to work correctly, all the ports should have the same power management settings before you create the team.

### Requirements for Express Teaming

- Microsoft Windows 2000, Windows XP, or Windows Server 2003

- A multi-port Intel® PRO/1000 adapter and driver where:

- None of the ports are disabled

- None of the ports are already teamed

- None of the ports are in a VLAN

- None of the ports have ASF enabled

| NOTES: If an adapter is configured for Express Teaming, performing Hot Plug operations with that adapter is not supported. The adapter becomes disabled. VLANs cannot be created on an Express Team, even if ANS is installed. Diagnostics are not supported for an Express Team. Identify Adapter blinks all ports of the Express Team. You can not access the individual ports in an Express Team.

## Adapter Settings

When an Express Team is created, only the initiator port remains visible. All other member ports are hidden. When the team is created, the settings for the secondary ports are saved and the settings for the initiator port are propagated throughout the team. When the team is disbanded, the primary port retains the settings made for the team and the secondary ports have their pre-team settings restored.

Once the team has been created, when you change a setting, it is changed for all ports in the team. The only exception is Locally Administered Address. This is a port-specific setting and is not propagated through the team.

`Last modified on 8/31/05 4:21p Revision 5`